From 91a74d361461494dd546467e83bc36c24185d6e7 Mon Sep 17 00:00:00 2001
From: Paul Eggert <eggert@cs.ucla.edu>
Date: Tue, 13 Jun 2023 21:10:24 -0700
Subject: [PATCH] wc: port to kernels that disable XSAVE YMM

Problem reported by Dave Hansen <https://bugs.gnu.org/64058>.
Apply similar change to cksum and pclmul, too.
* NEWS: Mention wc fix.
* configure.ac (cpuid_exists, get_cpuid_count_exists):
Remove.  All uses removed, since we no longer use __get_cpuid or
__get_cpuid_count.
(pclmul_intrinsic_exists, avx2_intrinsic_exists): Set to no if
__builtin_cpu_supports calls cannot be compiled.
(HAVE_PCLMUL_INTRINSIC, HAVE_AVX2_INTRINSIC): Remove; unused.
Simplify surrounding code because of this.
* src/cksum.c (pclmul_supported):
* src/wc.c (avx2_supported):
Use __builtin_cpu_supports instead of doing it by hand.
Simplify surrounding code because of this.

Reference:https://github.com/coreutils/coreutils/commit/91a74d361461494dd546467e83bc36c24185d6e7
Conflict:remove "a = _mm_shuffle_epi8 (a, b);" in configure.ac because it doesn't exist

---
 NEWS         |  3 +++
 configure.ac | 67 ++++++++--------------------------------------------
 src/cksum.c  | 26 +++++---------------
 src/wc.c     | 50 +++++----------------------------------
 4 files changed, 25 insertions(+), 121 deletions(-)

diff --git a/NEWS b/NEWS
index 7df9ff5b0..3350f9871 100644
--- a/NEWS
+++ b/NEWS
@@ -103,6 +103,9 @@ GNU coreutils NEWS                                    -*- outline -*-
   on (1024*5) buffer boundaries
   [bug introduced in coreutils-8.31]
 
+  'wc -l' no longer crashes on x86 Linux kernels that disable XSAVE YMM.
+  [bug introduced in coreutils-9.0]
+
 ** Changes in behavior
 
   cp and install now default to copy-on-write (COW) if available.
diff --git a/configure.ac b/configure.ac
index 520de8184..48dea9d01 100644
--- a/configure.ac
+++ b/configure.ac
@@ -527,27 +527,6 @@ CFLAGS=$ac_save_CFLAGS
 LDFLAGS=$ac_save_LDFLAGS
 ac_c_werror_flag=$cu_save_c_werror_flag
 
-AC_MSG_CHECKING([if __get_cpuid available])
-AC_LINK_IFELSE(
-  [AC_LANG_SOURCE([[
-    #include <cpuid.h>
-
-    int
-    main (void)
-    {
-      unsigned int eax, ebx, ecx, edx;
-      __get_cpuid (1, &eax, &ebx, &ecx, &edx);
-      return 1;
-    }
-  ]])
-  ],[
-    AC_MSG_RESULT([yes])
-    AC_DEFINE([HAVE_CPUID], [1], [__get_cpuid available])
-    cpuid_exists=yes
-  ],[
-    AC_MSG_RESULT([no])
-  ])
-
 ac_save_CFLAGS=$CFLAGS
 CFLAGS="-mavx -mpclmul $CFLAGS"
 AC_MSG_CHECKING([if pclmul intrinsic exists])
@@ -560,46 +539,23 @@ AC_COMPILE_IFELSE(
     {
       __m128i a, b;
       a = _mm_clmulepi64_si128 (a, b, 0x00);
-      return 1;
+      return __builtin_cpu_supports ("pclmul");
     }
   ]])
   ],[
-    AC_MSG_RESULT([yes])
-    AC_DEFINE([HAVE_PCLMUL_INTRINSIC], [1], [pclmul intrinsic exists])
     pclmul_intrinsic_exists=yes
   ],[
-    AC_MSG_RESULT([no])
+    pclmul_intrinsic_exists=no
   ])
-if test "x$cpuid_exists" = "xyes" &&
-   test "x$pclmul_intrinsic_exists" = "xyes"; then
+AC_MSG_RESULT([$pclmul_intrinsic_exists])
+if test $pclmul_intrinsic_exists = yes; then
   AC_DEFINE([USE_PCLMUL_CRC32], [1],
             [CRC32 calculation by pclmul hardware instruction enabled])
 fi
 AM_CONDITIONAL([USE_PCLMUL_CRC32],
-               [test "x$cpuid_exists" = "xyes" &&
-                test "x$pclmul_intrinsic_exists" = "xyes"])
+               [test $pclmul_intrinsic_exists = yes])
 CFLAGS=$ac_save_CFLAGS
 
-AC_MSG_CHECKING([if __get_cpuid_count exists])
-AC_LINK_IFELSE(
-  [AC_LANG_SOURCE([[
-    #include <cpuid.h>
-
-    int
-    main (void)
-    {
-      unsigned int eax = 0, ebx = 0, ecx = 0, edx = 0;
-      __get_cpuid_count (7, 0, &eax, &ebx, &ecx, &edx);
-      return 1;
-    }
-  ]])
-  ],[
-    AC_MSG_RESULT([yes])
-    get_cpuid_count_exists=yes
-  ],[
-    AC_MSG_RESULT([no])
-  ])
-
 CFLAGS="-mavx2 $CFLAGS"
 AC_MSG_CHECKING([if avx2 intrinstics exists])
 AC_COMPILE_IFELSE(
@@ -611,23 +567,20 @@ AC_COMPILE_IFELSE(
     {
       __m256i a, b;
       a = _mm256_sad_epu8 (a, b);
-      return 1;
+      return __builtin_cpu_supports ("avx2");
     }
   ]])
   ],[
-    AC_MSG_RESULT([yes])
-    AC_DEFINE([HAVE_AVX2_INTRINSIC], [1], [avx2 intrinsics exists])
     avx2_intrinsic_exists=yes
   ],[
-    AC_MSG_RESULT([no])
+    avx2_intrinsic_exists=no
   ])
-if test "x$get_cpuid_count_exists" = "xyes" &&
-   test "x$avx2_intrinsic_exists" = "xyes"; then
+AC_MSG_RESULT([$avx2_intrinsic_exists])
+if test $avx2_intrinsic_exists = yes; then
   AC_DEFINE([USE_AVX2_WC_LINECOUNT], [1], [Counting lines with AVX2 enabled])
 fi
 AM_CONDITIONAL([USE_AVX2_WC_LINECOUNT],
-               [test "x$get_cpuid_count_exists" = "xyes" &&
-                test "x$avx2_intrinsic_exists" = "xyes"])
+               [test $avx2_intrinsic_exists = yes])
 
 CFLAGS=$ac_save_CFLAGS
 
diff --git a/src/cksum.c b/src/cksum.c
index 85afab0ac..631ac3449 100644
--- a/src/cksum.c
+++ b/src/cksum.c
@@ -159,29 +159,15 @@ static bool
 pclmul_supported (void)
 {
 # if USE_PCLMUL_CRC32
-  unsigned int eax = 0;
-  unsigned int ebx = 0;
-  unsigned int ecx = 0;
-  unsigned int edx = 0;
-
-  if (! __get_cpuid (1, &eax, &ebx, &ecx, &edx))
-    {
-      if (cksum_debug)
-        error (0, 0, "%s", _("failed to get cpuid"));
-      return false;
-    }
-
-  if (! (ecx & bit_PCLMUL) || ! (ecx & bit_AVX))
-    {
-      if (cksum_debug)
-        error (0, 0, "%s", _("pclmul support not detected"));
-      return false;
-    }
+  bool pclmul_enabled = 0 < __builtin_cpu_supports ("pclmul");
 
   if (cksum_debug)
-    error (0, 0, "%s", _("using pclmul hardware support"));
+    error (0, 0, "%s",
+           (pclmul_enabled
+            ? _("using pclmul hardware support")
+            : _("pclmul support not detected")));
 
-  return true;
+  return pclmul_enabled;
 # else
   if (cksum_debug)
     error (0, 0, "%s", _("using generic hardware support"));
diff --git a/src/wc.c b/src/wc.c
index becceda98..3708d0b8f 100644
--- a/src/wc.c
+++ b/src/wc.c
@@ -132,52 +132,14 @@ static struct option const longopts[] =
 static bool
 avx2_supported (void)
 {
-  unsigned int eax = 0;
-  unsigned int ebx = 0;
-  unsigned int ecx = 0;
-  unsigned int edx = 0;
-  bool getcpuid_ok = false;
-  bool avx_enabled = false;
-
-  if (__get_cpuid (1, &eax, &ebx, &ecx, &edx))
-    {
-      getcpuid_ok = true;
-      if (ecx & bit_OSXSAVE)
-        avx_enabled = true;  /* Support is not disabled.  */
-    }
-
-
-  if (avx_enabled)
-    {
-      eax = ebx = ecx = edx = 0;
-      if (! __get_cpuid_count (7, 0, &eax, &ebx, &ecx, &edx))
-        getcpuid_ok = false;
-      else
-        {
-          if (! (ebx & bit_AVX2))
-            avx_enabled = false;  /* Hardware doesn't support it.  */
-        }
-    }
+  bool avx_enabled = 0 < __builtin_cpu_supports ("avx2");
 
+  if (debug)
+    error (0, 0, (avx_enabled
+                  ? _("using avx2 hardware support")
+                  : _("avx2 support not detected")));
 
-  if (! getcpuid_ok)
-    {
-      if (debug)
-        error (0, 0, "%s", _("failed to get cpuid"));
-      return false;
-    }
-  else if (! avx_enabled)
-    {
-      if (debug)
-        error (0, 0, "%s", _("avx2 support not detected"));
-      return false;
-    }
-  else
-    {
-      if (debug)
-        error (0, 0, "%s", _("using avx2 hardware support"));
-      return true;
-    }
+  return avx_enabled;
 }
 #endif
 
-- 
2.27.0

