From 28904d5266bc827b05ac1beb5e819878b56fc3f2 Mon Sep 17 00:00:00 2001
From: Wenkai Lin <linwenkai6@hisilicon.com>
Date: Sat, 23 Jul 2022 16:50:23 +0800
Subject: [PATCH 156/183] uadk: fix comment blank

Use 1 blank space(' ') instead of TAB('\t')
between the right comment and the previous code.

Signed-off-by: Wenkai Lin <linwenkai6@hisilicon.com>
---
 v1/drv/dummy_drv.c            | 4 ++--
 v1/internal/dummy_hw_usr_if.h | 2 +-
 v1/wd_util.h                  | 4 ++--
 3 files changed, 5 insertions(+), 5 deletions(-)

diff --git a/v1/drv/dummy_drv.c b/v1/drv/dummy_drv.c
index 206fa2b..f551b79 100644
--- a/v1/drv/dummy_drv.c
+++ b/v1/drv/dummy_drv.c
@@ -30,8 +30,8 @@
 
 struct dummy_q_priv {
 	int ver;
-	int head;		/* queue head */
-	int resp_tail;		/* resp tail in the queue */
+	int head;      /* queue head */
+	int resp_tail; /* resp tail in the queue */
 	/* so in the user side: when add to queue, head++ but don't exceed resp_tail.
 	 * when get back from the queue, resp_tail++ but don't exceed tail.
 	 * in the kernel side: when get from queue, tail++ but don't exceed head-1 */
diff --git a/v1/internal/dummy_hw_usr_if.h b/v1/internal/dummy_hw_usr_if.h
index c35f75d..3a9df48 100644
--- a/v1/internal/dummy_hw_usr_if.h
+++ b/v1/internal/dummy_hw_usr_if.h
@@ -35,7 +35,7 @@
 
 /* the format of the device io space, which is of drv */
 struct dummy_hw_queue_reg {
-	char hw_tag[DUMMY_HW_TAG_SZ];	/* should be "WDDUMMY\0" */
+	char hw_tag[DUMMY_HW_TAG_SZ];   /* should be "WDDUMMY\0" */
 	struct ring_bd ring[Q_BDS];	/* in real hardware, this is good to be
 					   in memory space, and will be fast
 					   for communication. here we keep it
diff --git a/v1/wd_util.h b/v1/wd_util.h
index d1642f8..e69b5f9 100644
--- a/v1/wd_util.h
+++ b/v1/wd_util.h
@@ -359,7 +359,7 @@ struct wcrypto_ecc_out {
 static inline void wd_reg_write(void *reg_addr, uint32_t value)
 {
 	*((uint32_t *)reg_addr) = value;
-	wmb();	/* load fence */
+	wmb(); /* load fence */
 }
 
 static inline uint32_t wd_reg_read(void *reg_addr)
@@ -367,7 +367,7 @@ static inline uint32_t wd_reg_read(void *reg_addr)
 	uint32_t temp;
 
 	temp = *((uint32_t *)reg_addr);
-	rmb();	/* load fence */
+	rmb(); /* load fence */
 
 	return temp;
 }
-- 
2.27.0

