From d0300cca906531d85d025c1c17a3d845a0f45902 Mon Sep 17 00:00:00 2001
From: Weili Qian <qianweili@huawei.com>
Date: Sat, 23 Jul 2022 10:49:00 +0800
Subject: [PATCH 174/183] drv/hpre: remove redundant blank line

This patch removes redundant blank line from the hpre driver.

Signed-off-by: Weili Qian <qianweili@huawei.com>
---
 drv/hisi_hpre.c | 1 -
 1 file changed, 1 deletion(-)

diff --git a/drv/hisi_hpre.c b/drv/hisi_hpre.c
index aea7749..d957101 100644
--- a/drv/hisi_hpre.c
+++ b/drv/hisi_hpre.c
@@ -771,7 +771,6 @@ static int ecc_prepare_alg(struct wd_ecc_msg *msg,
 	return 0;
 }
 
-
 static int trans_cv_param_to_hpre_bin(struct wd_dtb *p, struct wd_dtb *a,
 				      struct wd_dtb *b, struct wd_dtb *n,
 				      struct wd_ecc_point *g)
-- 
2.27.0

