From af330daeb1d215c312e0e4ff74cb4bc5f0f35cad Mon Sep 17 00:00:00 2001
From: Wenkai Lin <linwenkai6@hisilicon.com>
Date: Sun, 24 Apr 2022 09:54:25 +0800
Subject: [PATCH 120/183] uadk: fix switch statement has no default branch

msg->op_type is non-enumeral type '__u8', so switch statement
on it should have a default branch.

Signed-off-by: Wenkai Lin <linwenkai6@hisilicon.com>
---
 drv/hisi_hpre.c         | 3 ++-
 v1/drv/hisi_hpre_udrv.c | 2 ++
 2 files changed, 4 insertions(+), 1 deletion(-)

diff --git a/drv/hisi_hpre.c b/drv/hisi_hpre.c
index 33127e0..2a15900 100644
--- a/drv/hisi_hpre.c
+++ b/drv/hisi_hpre.c
@@ -1330,7 +1330,8 @@ static int ecc_prepare_out(struct wd_ecc_msg *msg, void **data)
 	case WD_SM2_KG:
 		*data = kout->pub.x.data;
 		break;
-	/* fall-through */
+	default:
+		break;
 	}
 
 	return ret;
diff --git a/v1/drv/hisi_hpre_udrv.c b/v1/drv/hisi_hpre_udrv.c
index bd87cbe..3d8a00f 100644
--- a/v1/drv/hisi_hpre_udrv.c
+++ b/v1/drv/hisi_hpre_udrv.c
@@ -1466,6 +1466,8 @@ static int qm_ecc_prepare_out(struct wcrypto_ecc_msg *msg, void **data)
 	case WCRYPTO_SM2_KG:
 		ret = ecc_prepare_sm2_kg_out(out, data);
 		break;
+	default:
+		break;
 	}
 
 	return ret;
-- 
2.27.0

