From d27c42baea5d52f3f4fdc36ed98c7d10289ad973 Mon Sep 17 00:00:00 2001
Message-Id: <d27c42baea5d52f3f4fdc36ed98c7d10289ad973.1488376602.git.dcaratti@redhat.com>
From: Sabrina Dubroca <sd@queasysnail.net>
Date: Sun, 27 Nov 2016 20:08:53 +0100
Subject: [PATCH] drivers: Move driver_wired_get_bssid() to a common file

This continues refactoring of the common parts of wired drivers code
into a shared file, so that they can be reused by other drivers.

Signed-off-by: Sabrina Dubroca <sd@queasysnail.net>
---
 src/drivers/driver_macsec_qca.c   | 10 +---------
 src/drivers/driver_wired.c        | 10 +---------
 src/drivers/driver_wired_common.c |  8 ++++++++
 src/drivers/driver_wired_common.h |  1 +
 4 files changed, 11 insertions(+), 18 deletions(-)

diff --git a/src/drivers/driver_macsec_qca.c b/src/drivers/driver_macsec_qca.c
index 15ea4bd..4bbc59f 100644
--- a/src/drivers/driver_macsec_qca.c
+++ b/src/drivers/driver_macsec_qca.c
@@ -83,14 +83,6 @@ static int macsec_qca_get_ssid(void *priv, u8 *ssid)
 }
 
 
-static int macsec_qca_get_bssid(void *priv, u8 *bssid)
-{
-	/* Report PAE group address as the "BSSID" for macsec connection. */
-	os_memcpy(bssid, pae_group_addr, ETH_ALEN);
-	return 0;
-}
-
-
 static void __macsec_drv_init(struct macsec_qca_data *drv)
 {
 	int ret = 0;
@@ -749,7 +741,7 @@ const struct wpa_driver_ops wpa_driver_macsec_qca_ops = {
 	.name = "macsec_qca",
 	.desc = "QCA MACsec Ethernet driver",
 	.get_ssid = macsec_qca_get_ssid,
-	.get_bssid = macsec_qca_get_bssid,
+	.get_bssid = driver_wired_get_bssid,
 	.get_capa = driver_wired_get_capa,
 	.init = macsec_qca_init,
 	.deinit = macsec_qca_deinit,
diff --git a/src/drivers/driver_wired.c b/src/drivers/driver_wired.c
index fd8a7e3..ad34627 100644
--- a/src/drivers/driver_wired.c
+++ b/src/drivers/driver_wired.c
@@ -374,14 +374,6 @@ static int wpa_driver_wired_get_ssid(void *priv, u8 *ssid)
 }
 
 
-static int wpa_driver_wired_get_bssid(void *priv, u8 *bssid)
-{
-	/* Report PAE group address as the "BSSID" for wired connection. */
-	os_memcpy(bssid, pae_group_addr, ETH_ALEN);
-	return 0;
-}
-
-
 static void * wpa_driver_wired_init(void *ctx, const char *ifname)
 {
 	struct wpa_driver_wired_data *drv;
@@ -415,7 +407,7 @@ const struct wpa_driver_ops wpa_driver_wired_ops = {
 	.hapd_deinit = wired_driver_hapd_deinit,
 	.hapd_send_eapol = wired_send_eapol,
 	.get_ssid = wpa_driver_wired_get_ssid,
-	.get_bssid = wpa_driver_wired_get_bssid,
+	.get_bssid = driver_wired_get_bssid,
 	.get_capa = driver_wired_get_capa,
 	.init = wpa_driver_wired_init,
 	.deinit = wpa_driver_wired_deinit,
diff --git a/src/drivers/driver_wired_common.c b/src/drivers/driver_wired_common.c
index b31474d..d30d3a4 100644
--- a/src/drivers/driver_wired_common.c
+++ b/src/drivers/driver_wired_common.c
@@ -164,6 +164,14 @@ int wired_multicast_membership(int sock, int ifindex, const u8 *addr, int add)
 }
 
 
+int driver_wired_get_bssid(void *priv, u8 *bssid)
+{
+	/* Report PAE group address as the "BSSID" for wired connection. */
+	os_memcpy(bssid, pae_group_addr, ETH_ALEN);
+	return 0;
+}
+
+
 int driver_wired_get_capa(void *priv, struct wpa_driver_capa *capa)
 {
 	os_memset(capa, 0, sizeof(*capa));
diff --git a/src/drivers/driver_wired_common.h b/src/drivers/driver_wired_common.h
index b926d83..493987a 100644
--- a/src/drivers/driver_wired_common.h
+++ b/src/drivers/driver_wired_common.h
@@ -26,6 +26,7 @@ int driver_wired_get_ifflags(const char *ifname, int *flags);
 int driver_wired_set_ifflags(const char *ifname, int flags);
 int driver_wired_multi(const char *ifname, const u8 *addr, int add);
 int wired_multicast_membership(int sock, int ifindex, const u8 *addr, int add);
+int driver_wired_get_bssid(void *priv, u8 *bssid);
 int driver_wired_get_capa(void *priv, struct wpa_driver_capa *capa);
 int driver_wired_get_ifstatus(const char *ifname, int *status);
 
-- 
2.7.4

