From e6009977b9ecb1136489b483e312a5e3e09a5497 Mon Sep 17 00:00:00 2001
From: Changsheng Wu <wuchangsheng2@huawei.com>
Date: Fri, 12 Nov 2021 17:04:22 +0800
Subject: [PATCH] huawei-0005-dpdk-change-the-log-level-in-prepare_numa

---
 lib/eal/linux/eal_memalloc.c | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

diff --git a/lib/eal/linux/eal_memalloc.c b/lib/eal/linux/eal_memalloc.c
index 337f2bc739..fc354f4a17 100644
--- a/lib/eal/linux/eal_memalloc.c
+++ b/lib/eal/linux/eal_memalloc.c
@@ -167,7 +167,7 @@ prepare_numa(int *oldpolicy, struct bitmask *oldmask, int socket_id)
 	RTE_LOG(DEBUG, EAL, "Trying to obtain current memory policy.\n");
 	if (get_mempolicy(oldpolicy, oldmask->maskp,
 			  oldmask->size + 1, 0, 0) < 0) {
-		RTE_LOG(ERR, EAL,
+		RTE_LOG(DEBUG, EAL,
 			"Failed to get current mempolicy: %s. "
 			"Assuming MPOL_DEFAULT.\n", strerror(errno));
 		*oldpolicy = MPOL_DEFAULT;
-- 
2.27.0

