From 44dd1455f924aa99e6bff0b124a9be0a85dcfa89 Mon Sep 17 00:00:00 2001
From: Peter Robinson <pbrobinson@gmail.com>
Date: Tue, 4 Sep 2018 11:59:18 +0100
Subject: [PATCH] rpi: Use firmware provided device tree

Signed-off-by: Peter Robinson <pbrobinson@gmail.com>
---
 configs/rpi_0_w_defconfig   | 2 +-
 configs/rpi_2_defconfig     | 2 +-
 configs/rpi_3_32b_defconfig | 2 +-
 configs/rpi_3_defconfig     | 2 +-
 configs/rpi_defconfig       | 2 +-
 5 files changed, 5 insertions(+), 5 deletions(-)

diff --git a/configs/rpi_0_w_defconfig b/configs/rpi_0_w_defconfig
index d5bf01b76e..08f177f34a 100644
--- a/configs/rpi_0_w_defconfig
+++ b/configs/rpi_0_w_defconfig
@@ -13,7 +13,7 @@ CONFIG_SYS_PROMPT="U-Boot> "
 CONFIG_CMD_GPIO=y
 CONFIG_CMD_MMC=y
 CONFIG_CMD_USB=y
-CONFIG_OF_EMBED=y
+CONFIG_OF_BOARD=y
 CONFIG_DEFAULT_DEVICE_TREE="bcm2835-rpi-zero-w"
 CONFIG_ENV_FAT_INTERFACE="mmc"
 CONFIG_ENV_FAT_DEVICE_AND_PART="0:1"
diff --git a/configs/rpi_2_defconfig b/configs/rpi_2_defconfig
index a50a815759..0918c6c9ff 100644
--- a/configs/rpi_2_defconfig
+++ b/configs/rpi_2_defconfig
@@ -13,7 +13,7 @@ CONFIG_SYS_PROMPT="U-Boot> "
 CONFIG_CMD_GPIO=y
 CONFIG_CMD_MMC=y
 CONFIG_CMD_USB=y
-CONFIG_OF_EMBED=y
+CONFIG_OF_BOARD=y
 CONFIG_DEFAULT_DEVICE_TREE="bcm2836-rpi-2-b"
 CONFIG_ENV_FAT_INTERFACE="mmc"
 CONFIG_ENV_FAT_DEVICE_AND_PART="0:1"
diff --git a/configs/rpi_3_32b_defconfig b/configs/rpi_3_32b_defconfig
index ec395d29ed..22165bde53 100644
--- a/configs/rpi_3_32b_defconfig
+++ b/configs/rpi_3_32b_defconfig
@@ -14,7 +14,7 @@ CONFIG_SYS_PROMPT="U-Boot> "
 CONFIG_CMD_GPIO=y
 CONFIG_CMD_MMC=y
 CONFIG_CMD_USB=y
-CONFIG_OF_EMBED=y
+CONFIG_OF_BOARD=y
 CONFIG_DEFAULT_DEVICE_TREE="bcm2837-rpi-3-b"
 CONFIG_ENV_FAT_INTERFACE="mmc"
 CONFIG_ENV_FAT_DEVICE_AND_PART="0:1"
diff --git a/configs/rpi_3_defconfig b/configs/rpi_3_defconfig
index ac99f2000a..0ca298cd54 100644
--- a/configs/rpi_3_defconfig
+++ b/configs/rpi_3_defconfig
@@ -14,7 +14,7 @@ CONFIG_SYS_PROMPT="U-Boot> "
 CONFIG_CMD_GPIO=y
 CONFIG_CMD_MMC=y
 CONFIG_CMD_USB=y
-CONFIG_OF_EMBED=y
+CONFIG_OF_BOARD=y
 CONFIG_DEFAULT_DEVICE_TREE="bcm2837-rpi-3-b"
 CONFIG_ENV_FAT_INTERFACE="mmc"
 CONFIG_ENV_FAT_DEVICE_AND_PART="0:1"
diff --git a/configs/rpi_defconfig b/configs/rpi_defconfig
index db42ffd135..0ec1365b1b 100644
--- a/configs/rpi_defconfig
+++ b/configs/rpi_defconfig
@@ -13,7 +13,7 @@ CONFIG_SYS_PROMPT="U-Boot> "
 CONFIG_CMD_GPIO=y
 CONFIG_CMD_MMC=y
 CONFIG_CMD_USB=y
-CONFIG_OF_EMBED=y
+CONFIG_OF_BOARD=y
 CONFIG_DEFAULT_DEVICE_TREE="bcm2835-rpi-b"
 CONFIG_ENV_FAT_INTERFACE="mmc"
 CONFIG_ENV_FAT_DEVICE_AND_PART="0:1"
-- 
2.19.0.rc0

